Pins for Huzzah from top: na | TX | RX | V+ | na | GND

Must remove blue pin # 16 when flashing (for sleep reset)

Project runs at 3v3. Solar puts in 6v. Bat 4.2v 1200mAh (rated 3v7)

Uses SHT11 Sensiron temp and humidity sensor. With 10K R on one of the lines (think data)

Charger: <https://www.adafruit.com/product/259>

PWR Supply: <http://www.banggood.com/5Pcs-Mini-DC-Adjustable-Power-Supply-Buck-Module-Step-Down-Module-p-952402.html>

Sketch: WeatherStation5TX.ino